> # Default Settings

> Table 17-5 lists the default settings for basic zone parameters.

> Table 17-5 Default Basic Zone Parameters
> Parameters | Default
> --- | ---
> Default zone policy | Denied to all members.
> Full zone set distribute | The full zone set(s) is not distributed.
> Zone based traffic priority | Low.
> Read-only zones | Read-write attributes for all zones.
> Broadcast frames | Sent to all Nx ports.
> Broadcast zoning | Disabled.
> Enhanced zoning | Disabled.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.