> # Port Security Active Database

> Field | Description
> --- | ---
> Interface or fWWN | The address of a port on the local device.
> Type | The mechanism to identify a switch port. fwwn— The local switch port is identified by Fabric WWN(fWWN). intfIndex— The local switch port is identified by ifIndex. wildCard—Wild card (any switch port on local device).
> WWN | Represents the logging-in device address.
> IsLearnt | Indicates if this entry is a learned entry or not.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.