> # Mapping Fabric ID to Server ID

> The IP address of the physical server will be mapped to the server ID during the installation of the Cisco DCNM-SAN Server whenever the IP address of the physical server is changed, you need to map the IP address to the server ID using the PLMapping script provided with the Cisco DCNM-SAN Server. Whenever the you open or discover a fabric, the fabric ID will be mapped to the server ID . You can move a fabric to a different server ID using the control panel.

> ## DETAILED STEPS

> 1. Choose Server > Admin.

> You see the Control Panel.

> 2. Select the fabric that you want to move to a different server and then click Move.

> You see the Move Fabric dialog box.

> 3. You see the fabrics that you selected in the Fabrics to Move list box. From the Move To Server drop-down list select the server you want to move the fabric to.
> 4. Click Move.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.