> # Creating a Class Map

> Detailed StepsTo create a class map using Fabric Manager, follow these steps:

> 1. Expand Switches, expand FC Services and then select QoS in the Physical Attributes pane.

> The QoS information is displayed in the Information pane. The Control tab is the default.

> 2. In the Class Maps tab, click Create Row to create a new class map.

> You see the Create Class Maps dialog box.

> 3. Select the switches for the class map.
> 4. Enter the source ID or the destination ID in the field.
> 5. Enter a name for the class map.
> 6. Select a Match mode.You can either match any or all criterion with one match statement from the class map configuration mode.
> 7. Click Create to proceed with creating the class map.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.