> # Converting to Manually Configured Channel Groups

> To convert an autocreated channel group to a user-configured channel group using DCNM-SAN, follow these steps:

> 1. Expand ISLs and then select Port Channels in the Physical Attributes pane.
> 2. Click the Protocol tab.

> You see the switch protocols.

> 3. Check the Persist check box for each channel that you want to convert to a manually configured channel group.
> 4. Click the Apply Changes icon to save any modifications.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.