Settings

1. From the menu bar, choose Health> SAN Host Redundancy> Settings.

2. Under the Test for pane, use the check boxes to select the host redundancy optional checks.

3. For accurate results in hosts with LUN mismatch check, perform a purge under SMIS discovery in data sources page to remove any LUNs that were discovered earlier but are no longer visible.

4. Select the Automatically Run Check Every 24 hours checkbox to enable periodic running of the checker. The checker will run every 24 hours starting 10 minutes after the server starts.

5. The Ignored Hosts pane displays the list of host enclosures that have been skipped/ignored by the redundancy check along with the reason the host enclosure check was skipped.The following reasons may be displayed:

• Enclosure has only one HBA

• Host was ignored by the user.

• Host ports managed by more than one federated server.

• No path storage found.

6. The Host Enclosure column displays the ignored hosts. Click a host to view the Compute details.

7. Select a host enclosure and click the Delete button to remove the host from the ignored list and begin receiving errors about a host you had chosen to ignore. However, you cannot delete ignored hosts if they were ignored because:

• They did not have at least two ports.

• They were managed by two or more federated servers.