> # Clearing Sessions

> ## Detailed Steps

> To clear a RADIUS or TACACS+ distribution, follow these steps:

> 1. Expand Switches > Security > AAA and then select either RADIUS or TACACS+.

> You see either the RADIUS or TACACS+ configuration in the Information pane.

> 2. Choose the CFS tab. You see either the RADIUS or TACACS+ CFS configuration.
> 3. Choose clear from the Config Action drop-down list for each switch that should clear the pending RADIUS or TACACS+ distribution.
> 4. Click Apply Changes.
> .

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.