Configuring SFTP

You can configure the SFTP credentials for a switch.

1. From the menu bar, choose Admin > General > SFTP/TFTP Credentials.
You see the SFTP/TFTP credentials page.

2. In the Server Type field, use the radio button to select SFTP.

3. Enter the SFTP Username and SFTP Password.

4. Enter the Root Directory path.

5. From the Verification Switch drop-down, select the switch.

6. Click Apply to apply the configuration.

7. Click Apply and Verify to apply and verify the configuration.

8. Click Clear SSH Hosts to clear SSH hosts for all switches or selected switches. If there is a failure in any of the switches, an error message is displayed. Go to Admin>Logs>Web Report to view the number of successful and unsuccessful switches.