> # Changing the IP Address of the Cisco DCNM-SAN Server

> ## DETAILED STEPS

> 1. Stop the Cisco DCNM-SAN Server.
> 2. Change the following parameter in the $INSTALLDIR/conf/FMServer.conf.

> wrapper.app.parameter.4=127.0.0.1

> 3. Change the following parameter in the $INSTALLDIR/conf/server.properties.

> server.bindaddrs = 127.0.0.1

> 4. Enter the following command to assign a new IP address.

>     run $INSTALLDIR/bin/PLMapping.bat -p newipaddress 0

> Assume $INSTALLDIR is the top directory of DCNM-SAN installation. The above command is for single server instance, where 0 is the server ID.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.