> # Committing Changes

> To apply the pending domain configuration changes to other MDS switches in the VSAN, you must commit the changes. The pending configuration changes are distributed and, on a successful commit, the configuration changes are applied to the active configuration in the MDS switches throughout the VSAN and the fabric lock is released.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.