> # Deleting an Interface from a PortChannel

> ## Detailed Steps

> To delete a physical interface (or a range of physical interfaces) from a PortChannel using DCNM-SAN, follow these steps:

> 1. Expand ISLs and then select Port Channels in the Physical Attributes pane.

> You see the PortChannels in the Information pane.

> 2. Click the Channels tab and find the switch and PortChannel that you want to edit.
> 3. Remove the interface or list of interfaces you want deleted in the Members the Admin column.
> 4. Click the Apply Changes icon to save any modifications.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.