> # Port Security Database Differences

> Field | Description
> --- | ---
> CompareWith | Specifies the database for the comparison. configDb— Compares the configuration database with respect to active database on this VSAN/VLAN. So, the active database will be the reference database and the results of the difference operation will be with respect to the active database. activeDb— Compares the active database with respect to configuration database on this VSAN/VLAN. So, the configuration database will be the reference database and the results of the difference operation will be with respect to the configuration database.
> VSANId | The ID of the VSAN to compare against.
> Interface/fWWN | The address of a port on the local device.
> Type | The mechanism to identify a switch port. fwwn— The local switch port is identified by Fabric WWN(fWWN). intfIndex— The local switch port is identified by ifIndex. wildCard— Wild card (any switch port on local device).
> WWN | Represents the logging in device address.
> Reason | Indicates the reason for the difference between the databases being compared, for this entry.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.