> # Resetting FSPF to the Default Configuration

> ## Detailed Steps

> To return the FSPF VSAN global configuration to its factory default, follow these steps:

> 1. Expand a Fabric, expand a VSAN, and select FSPF for a VSAN that you want to configure for FSPF.

> You see the FSPF configuration in the Information pane.

> 2. Check the SetToDefault check box for a switch.
> 3. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.