> # Creating Crypto Map Entries

> ## Detailed Steps

> To create mandatory crypto map entries, follow these steps:

> 1. Expand Switches > Security, and then select IPSEC in the Physical Attributes pane.
> 2. Click the CryptoMap Set Entry tab.
> 3. (Optional) Click Create Row to create a crypto map entry.
> 4. Select the switch that you want to configure or modify. If you are creating a crypto map, set the setName and priority for this crypto map.
> 5. Select the IPv4-ACL Profile and TransformSetIdList from the drop-down list for this crypto map.
> 6. (Optional) Check the AutoPeer check box or set the peer address if you are creating a crypto map. See the "About the AutoPeer Option" topic.
> 7. Choose the appropriate PFS selection. See the "About Perfect Forward Secrecy" topic.
> 8. Supply the Lifetime and LifeSize. See the "About SA Lifetime Negotiation" topic.
> 9. Click Create if you are creating a crypto map, or click Apply Changes if you are modifying an existing crypto map.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.