> # Disruptive

> Disruptive load balance works independent of automatic selection of interfaces and a configured traffic map of external interfaces. This feature forces reinitialization of the server interfaces to achieve load balance when this feature is enabled and whenever a new external interface comes up. To avoid flapping the server interfaces too often, enable this feature once and then disable it whenever the needed load balance is achieved.

> If disruptive load balance is not enabled, you need to manually flap the server interface to move some of the load to a new external interface.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.