> # Configuring Cisco DCNM-SAN Server Properties

> To configure Cisco DCNM-SAN Server properties

> 1. From the menu bar, choose Admin > General > Server Properties.
> 2. Follow the on-screen instructions and click Apply to confirm the changes.

> While connecting to some switches if the connection is getting timed out, in the #CLI session channel type, change default the cli.channel.type value from exec to shell.

> Note After configuring the server properties, you need to restart the DCNM server only if you receive a notification stating that the server must be restarted.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.