> # Security Role Rules

> Note: this table applies only to Nexus 5000 Series switches.

> Field | Description
> --- | ---
> Rule Order | The rules are applied in numerical order.
> Permit? | Indicates whether the rule will permit or deny the operation.
> Rule Operation | The rule can specify read-only access or read-write access to the operation.
> Rule Element Type | The rule can be applied to a command, a feature, feature group or all. Select all to apply the rule to all commands and features.
> Rule Element | The rule element specifies the command, feature or feature group to which the rule applies.
> Features/Groups | Click the Features/Groups button to open the feature group manager.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.