> # Configuring SNMPv2c Notifications

> ## Detailed Steps

> To configure SNMPv2c notifications, follow these steps:

> 1. Expand Events and then select SNMP Traps in the Physical Attributes pane.

> You see the SNMP notification configuration in the Information pane.

> 2. Click the Destinations tab to add or modify a receiver for SNMP notifications.
> 3. Click Create Row to create a new notification destination.

> You see the Create Destinations dialog box.

> 4. Check the switches for which you want to configure a new destination.
> 5. Set the destination IP address and UDP port.
> 6. Choose either the trap or inform radio button.
> 7. (Optional) Set the timeout or retry count values.
> 8. Click Create to add this destination to the selected switches.
> 9. (Optional) Click the Other tab to enable specific notification types per switch.
> 10. Click the Apply changes icon to create the entry.

> Note Switches can forward events (SNMP traps and informs) up to 10 destinations.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.