> # Registering Name Server Proxies

> ## Detailed Steps

> To register the name server proxy, follow these steps:

> 1. Expand a fabric, expand a VSAN, and then select Advanced.

> You see the VSAN advanced configuration in the Information pane.

> 2. Click the NS Proxies tab.

> You see the existing name server proxy for the selected VSAN.

> 3. Double-click the PortName field to register a new name server proxy.
> 4. Click Apply Changes to save these changes, or click Undo Changes to cancel any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.