> # Clearing a Fabric Lock

> If you have performed an iSLB configuration task and have not released the lock by either committing or discarding the changes, an administrator can release the lock from any switch in the fabric. If the administrator performs this task, your pending changes are discarded and the fabric lock is released.

> ## Restrictions

> The pending changes are only available in the volatile directory and are discarded if the switch is restarted.

> ## Detailed Steps

> To release a fabric lock using Device Manager, follow these steps:

> 1. Choose Admin > CFS.

> You see the CFS Configuration dialog box.

> 2. Set the Command field to clear for the iSLB feature.
> 3. Click Apply to save this change.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.