> # Creating an FCS Platform

> ## Detailed Steps

> To create an FCS platform, follow these steps:

> 1. Choose FC > Advanced > Fabric Config Server.

> You see the Fabric Config Server dialog box.

> 2. Click the Platforms (Enclosures) tab.
> 3. Click Create.

> You see the Create Fabric Config Server dialog box.

> 4. Enter the VSAN ID, or select the ID from the drop-down list of available VSAN IDs.
> 5. Enter the Fabric Configuration Server name in the Name field.
> 6. Choose the type of server (Gateway, Host, Storage).
> 7. Enter the WWNs for the server.
> 8. Enter the management addresses for the server.
> 9. Click Create to create the server, or click Close to discard your changes and return to the Fabric Config Server dialog box.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.