> # New Area - Daily Performance

> This area displays the total performance of the displayed scope broken into three sections. ISL, Host and Storage. Total monitored port count per area is shown below the circular graph.

> Each of the circular graphs will display the percentage of utilization based on 3 different thresholds depicted with color differentiation as follows:

> - 0-50%: Green
> - 51-80%: Yellow
> - 81-100%: Red

> You can click each displayed area to view performance data for only the ports, which fall within each performance scope. This will display more detailed information on each entry by displaying the name of the port. Click the bar graph icon to display the historical performance data for the selected port. A full performance graph also appears on the bottom of the screen displaying the last 24 hours, week, month, and year.

> You can switch the graph to be displayed as a histogram and to perform predictive analysis on the port showing the most likely performance over the next 6 months based on the historical data gathered for the port. Click the + icon in the bar graph to overlay the performance data of any other port by clicking on the + icon and then clicking the graph icon next to another port listed above. The VSAN/VLAN configuration, speed of the trunk/ISL the average and peak receive data, the average and peak transmit data, the combined receive and transmit, the total number of errors and discards in the last 24 hours, and the last time the data was updated are also displayed.

> To return to the summary view, from the menu bar select Dashboard>Network.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.