> # Default Settings

> Table 30-2 lists the default settings for all switch security features in any switch.

> Table 30-2 Default Switch Security Settings
> Parameters | Default
> --- | ---
> Roles in Cisco MDS switches | Network operator (network-operator)
> AAA configuration services | Local
> Authentication port | 1812
> Accounting port | 1813
> Preshared key communication | Clear text
> RADIUS server timeout | 1 (one) second
> RADIUS server retries | Once
> Authorization | Disabled
> aaa user default role | enabled
> RADIUS server directed requests | Disabled
> TACACS+ | Disabled
> TACACS+ servers | None configured
> TACACS+ server timeout | 5 seconds
> TACACS+ server directed requests | Disabled
> AAA server distribution | Disabled
> Accounting log size | 250 KB

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.