> # IPSEC Global

> Field | Description
> --- | ---
> Lifetime (sec) | The default lifetime (in seconds) assigned to an IPsec tunnel as a global policy (maybe overridden in specific cryptomap definitions).
> Lifesize (KB) | The default life size in KB assigned to an IPsec tunnel as a global policy (unless overridden in cryptomap definition).

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.