> # Clearing a Fabric Lock

> To release a fabric lock, follow these steps:

> 1. Expand Fabric > All VSANs > Domain Manager and then select AllowedId in the Logical Domains pane for the fabric and VSAN for which you want the allowed domain ID list.

> You see the CFS configuration in the Information pane.

> 1. Set the Config Action drop-down menu to clear.
> 2. Click the Apply Changes icon to clear the fabric lock.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.