> # Fabric Binding Violations

> Field | Description
> --- | ---
> Peer WWN | The sWWN (switch WWN) of the device that was denied entry into the fabric on one of the local device's ports.
> DomainId | The domain ID of the device that was denied entry into the fabric on one of the local device's ports. A value of zero indicates that the switch WWN of the device was not present in the enforced fabric bindings.
> DenialTime | When the denial took place.
> DenialCount | The number of times this switch has been denied entry into the fabric on one of the local device's ports.
> DenialReason | The reason for which the device was denied entry into the fabric on one of the local device's ports.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.