> # SDV Virtual Devices

> Field | Description
> --- | ---
> Name | Represents the name of this virtual device.
> Virtual Domain | The user preference for a persistent Domain ID for this virtual device to indicate a specific partition (domain) of the fabric that this virtual device should belong to.
> Virtual FCID | The user preference for a persistent FCID for this virtual device.
> Port WWN | The assigned PWWN for this virtual device. The agent assigns this value when the configuration is committed.
> Node WWN | The assigned NWWN for this virtual device. The agent assigns this value when the configuration is committed.
> Assigned FCID | The assigned FCID of this virtual device. The agent assigns this value when the configuration is committed and the real device that this virtual device virtualizes is on-line.
> Real Device Map List | The set of real device(s) that this virtual device virtualizes in this VSAN.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.