> # Committing Changes

> If you commit the changes made to the configuration, the configuration in the DPVM pending database are distributed to other switches. On a successful commit, the configuration change is applied throughout the fabric and the lock is released.

> ## Detailed Steps

> To commit the DPVM pending database, follow these steps:

> 1. Expand Fabric xx> All VSANs, and then select DPVM from the Logical Attributes pane.

> You see the DPVM configuration in the Information pane.

> 2. Click the CFS tab and select commit from the Config Action drop-down menu.
> 3. Click Apply Changes to save this change or click Undo Changes to discard the change.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.