> # Settings

> 1. From the menu bar, choose Health> SAN Host Redundancy> Settings.
> 2. Under the Test for pane, use the check boxes to select the host redundancy optional checks.
> 3. Select the Automatically Run Check Every 24 hours checkbox to enable periodic running of the checker. The checker will run every 24 hours starting 10 minutes after the server starts.
> 4. The Ignored Hosts pane displays the list of host enclosures that have been skipped/ignored by the redundancy check along with the reason the host enclosure check was skipped.The following reasons may be displayed:
> - Enclosure has only one HBA
> - Host was ignored by the user.
> - Host ports managed by more than one federated server.
> - No path to storage found.
> 5. The Host Enclosure column displays the ignored hosts. Click a host to view the Compute details.
> 6. Select a host enclosure and click the Delete button to remove the host from the ignored list and begin receiving errors about a host you had chosen to ignore. However, you cannot delete ignored hosts if they were ignored because:
> - They did not have at least two ports.
> - They were managed by two or more federated servers.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.