> # DPVM Active Database

> Field | Description
> --- | ---
> Type | Specifies the type of the corresponding instance of cdpvmEnfLoginDev.
> WWN or Name or MAC | Represents the logging in device. The value depends on the corresponding device type (PWWN, NWWN or MAC).
> VSAN Id | Represents the VSAN of the port on the local device through which the device represented by cdpvmEnfLoginDev logs in.
> Interface | Represents the device alias.
> IsLearnt | Indicates whether this is a learnt entry or not. If true, then it is a learnt entry. If false, then it is not.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.