> # New Area - Topology

> This displays the current physical topology with color- coding (displayed with a key in the lower right corner) for ISL utilization. You can hover over the switch indication circles to display the configured switch name, IP address, switch model, firmware version, last polled CPU utilization, and last polled memory utilization.

> You can toggle to display memory or CPU utilization on the switch indicators, by clicking the memory or CPU tachometer in the upper left corner in the topology map to display peak utilization for the last 24 hours on those switches. In addition the ISL/Trunk paths are also color-coded based on their TX+RX peak utilization. You can hover over the ISL/Trunk to show list of ports that create the connection and click on individual paths to launch the performance chart showcasing TX and RX utilization for the last 24 hours.

> Click the + symbol in the upper-right corner to maximize the window and enables you to drag the switch icons to best display their infrastructure. Once icons are placed in the most desirable position you can save the layout by clicking the Save icon in the upper-left corner of the topology map. If the layout is moved you can restore the previously saved layout during the current session by clicking the Restore icon in the upper-left corner next to the save icon.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.