> # Configuring Domain Parameters

> The Fibre Channel domain (fcdomain) feature performs principal switch selection, domain ID distribution, FC ID allocation, and fabric reconfiguration functions as described in the FC-SW-2 standards.

> This chapter includes the following sections:

> - Information About Fibre Channel Domains
> - Guidelines and Limitations
> - Default Settings
> - Configuring Fibre Channel Domains
> - Configuring Domain IDs
> - Configuring FC IDs
> - Verifying FC Domain Configuration
> - Monitoring FC Domain
> - Field Descriptions for FC Domain
> - Feature History for Domain Parameters

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.