> # Zoneset Enhanced

> Field | Description
> --- | ---
> Action | When set to basic(1), results in the zone server operating in the basic mode as defined by FC-GS4 standards. When set to enhanced(2), results in the zone server operating in the enhanced mode as defined by FC-GS4 standards.
> Result | The outcome of setting the mode of operation of the local Zone Server on this VSAN.
> Config DB Locked By | Specifies the owner for this session.
> Config DB Discard Changes | Assists in committing or clearing the contents of the copy database on this session.
> Config DB Result | Indicates the outcome of setting the corresponding instance of czseSessionCntl to commitChanges(1).
> Enforce Full DB Merge | Controls the zone merge behavior. If this object is set to allow, then the merge takes place according to the merge rules. If set to restrict, then if the merging databases are not exactly identical, the Inter-Switch Link (ISL) between the devices is isolated.
> Read From | Specifies whether the management station wishes to read from the effective database or from the copy database.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.