> # Configuring Domain Manager Turbo Mode

> The Domain Manager turbo mode feature allows you to restart the Domain Manager with optimization. You have the option to select fast-restart or selective-restart mode for restarting the Domain Manager. You can leave the restart mode empty indicating that optimization is disabled.

> ## Detailed Steps

> To configure the Domain Manager turbo mode, follow these steps:

> 1. Expand Fabric > All VSANs and then select Domain Manager in the Logical Domains pane for the fabric and VSAN for which you want to configure turbo mode.
>    You see the Running tab configuration of the domain in the Information pane.
> 2. Click the Configuration tab.
> 3. Set the Optimization drop-down menu to fast-restart or selective-restart for any switch in the fabric that you want to optimize. You can leave the Optimization field without any selection, indicating that the optimization is disabled.
> 4. Click the Apply Changes icon to initiate this restart.

> To configure the Domain Manager turbo mode using Device Manager, follow these steps:

> 1. Expand FC > Domain Manager and then select the Configuration tab.

> Note The Optimization field is not available in releases prior to NX-OS Release 4.2(1).

> 2. Set the Optimization drop-down menu to fast-restart or selective-restart for any switch in the fabric that you want to optimize. You can leave the Optimization field without any selection, indicating that the optimization is disabled.
> 3. Click Apply to initiate this restart.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.