> # RMON Thresholds Events

> Field | Description
> --- | ---
> Description | A comment describing this event entry.
> Type | The type of notification that the probe will make about this event. In the case of log, an entry is made in the log table for each event. In the case of SNMP-trap, an SNMP trap is sent to one or more management stations.
> Community | The community string.
> LastTimeSent | When this event entry last generated an event. If this entry has not generated any events, this value will be N/A.
> Owner | The entity that configured this entry and is therefore using the resources assigned to it.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.