> # Configuring the Initiator Version

> ## Detailed Steps

> To configure the initiator version, follow these steps:

> 1. Expand Switches > Security, and then select IKE.
> 2. Click the Initiator Version tab.

> You see the existing initiator versions for the peers in the Information pane.

> 3. Click Create Row to create an initiator version.
> 4. Select the Switches for the remote peer for which this IKE protocol initiator is configured.
> 5. Enter the IP address of the remote peer.

> IKEv1 represents the IKE protocol version used when connecting to a remote peer.

> 6. Click Create to create this initiator version or click Close to discard any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.