> # Default Settings

> Table 32-2 lists the default settings for all fabric security features in any switch.

> Table 32-2 Default Fabric Security Settings
> Parameters | Default
> --- | ---
> DHCHAP feature | Disabled
> DHCHAP hash algorithm | A priority list of MD5 followed by SHA-1 for DHCHAP authentication
> DHCHAP authentication mode | Auto-passive
> DHCHAP group default priority exchange order | 0, 4, 1, 2, and 3 respectively
> DHCHAP timeout value | 30 seconds

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.