> # Interface Port Monitoring Protocol

> The Monitor dialogs have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> OlsIns | The number of Offline Sequence errors received by the FC-Port.
> OlsOuts | The number of Offline Sequence errors issued by the FC-Port.
> LinkResetIns | The number of link reset protocol errors received by the FC-Port from the attached FC-port.
> LinkResetOuts | The number of link reset protocol errors issued by the FC-Port to the attached FC-Port.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.