> # FC Interfaces FICON Peer

> Field | Description
> --- | ---
> TypeNumber | The type number of the peer node. For example, the type number could be 002105.
> SerialNumber | The sequence number assigned to the peer node during manufacturing. For example, the serial number could be 000000023053.
> Tag | The identifier of the port in the peer node connected to this port.
> FcId | Address Identifier assigned to NX-Port
> Status | Specifies the status of the row, is valid, invalid or old.
> Name | Name of this port.
> Manufacturer | The name of the company that manufactured the peer node. For example, the manufacturer info could be HTC.
> ModelNumber | The model number of the peer node. For example, the model number could be F20.
> PlantOfMfg | The plant code that identifies the plant of manufacture of the peer node. For example, the plant code of manufacture could be 00.
> UnitType | The type of the peer node that this port is communicating.
> Alert | The type of link incident that occurred on this interface.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.