# Border Leaf Extended Partitions

This screen lists the extended partitions, selected Border Leaf/Edge Router pairs, and their corresponding profiles and configurations. From the menu bar, select Config > Extended Partitions.

The following icons are listed at the menu bar of the window to customize the view of the information in the window:

Field | Description
VRF | Specifies the VRF name for the extended partition.
Organization | Specifies the name of organization which the extended partition belongs to.
Partition | Specifies the name of the partition that is extended.
Redundancy Factor | Specifies the run-time redundancy factor for that partition extension.
Edge Router | Specifies the name of the Edge Router.
Edge Router IP Address | Specifies the IP address of the Edge Router device.
Edge Router Profile | Specifies the default profile for the edge router.
Border Leaf (BL) | Specifies the name of the Border Leaf device
BL IP Address | Specifies the IP address of the Border Leaf device.
BL Profile | Specifies the default profile for the border leaf device.