> # Assigning SNMP Switch Contact and Location Information

> You can assign the switch contact information, which is limited to 32 characters (without spaces), and the switch location.

> ## Detailed Steps

> To configure contact and location information, follow these steps:

> 1. Expand Switches from the Physical Attributes pane.

> You see the switch settings in the Information pane.

> 2. Fill in the Location and Contact fields for each switch.
> 3. Click Apply Changes to save these changes or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.