cfgfmt version 2.3

This tool is used to create binary profile from input text
profile (derived from one of sip_example.txt, sccp_example.txt,
h323_example.txt, or mgcp_example.txt template text profile
distributed with CCO image package) that Cisco ATA or Cisco IP
Phone 7902/7905/7912 accepts in TFTP profile download. For detail
on its usage, please refer to the respective administrator guide
of the platform and protocol of interest. This tool also requires
the appropriate "ptag.dat" file as its input. Please use
the correct "ptag.dat" file along with the corresponding
template text profile that are distributed as part of the
CCO image package of interest.


cfgfmt version 2.3
usage: cfgfmt [options] input output
options:
	-eRc4Passwd -- use Rc4Passwd to encrypt or decrypt input
	-E -- do not use EncryptKey parameter's value in the input
	      text file to encrypt the output binary file
	-xRc4Passwd -- use stronger Rc4Passwd to encrypt or decrypt input,
		RC4Passwd entered must be in hex
	-X -- do not use EncryptKeyEx parameter's value in the input
	      text file to encrypt the output binary file
	-tPtagFile -- specify an alternate PtagFile path
	-sip -- limit to sip protocol parameters
	-h323 -- limit to h323 protocol parameters
	-mgcp -- limit to mgcp procotol parameters
	-sccp -- limit to sccp protocol parameters
	-g -- omit sensitive parameters in old ata<mac> file

