swrvcon(1)

NAME
swrvcon - Virtual console for Cisco's IOS-Linux based software router

SYNOPSIS
swrvcon [OPTIONS] [instance]

DESCRIPTION
swrvcon is an optional virtual console to Cisco's IOS Linux based software router. It allows a user to connect and disconnect to a software router instance multiple times. The Control-C should be used to exit the the swrvcon application.

COMMAND-LINE OPTIONS

-d  Enable debug traces

-h  Display this help

-v  Display version information

EXAMPLES

$ sudo ./swrvcon 100
    This command uses the swrvcon application to access the Cisco IOS Linux based software router command-line interface (CLI). The 100 identifies the software router application ID. Once the user has access, the IOS configuration can be managed.

$ sudo ./swrvcon 100 &
    This command runs the swrvcon application in the background, if desired.

PREREQUISITE
The Software Router command line option, -L, must be specified when the application is launched. The example below shows the -L option. $ sudo ./i86bi_swr-universalk9-ms -e 1 -L 100

SEE ALSO

COPYRIGHT
Copyright (c) 2011 by Cisco systems, Inc.