BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0163
RTR from extension enabled ?

The command defines whether or not an extension should be allowed to initiate calls to other guest rooms (RTR calls). The command is valid for hotel guest room extensions only!

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003