BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5506
Delete call pickup ext. group

In ASB 150 a call pickup group is formed from a list of extensions. In case of a call to a member of the group another member can answer the call from his/her own telephone by dialling the code for “group call pickup”.

With this command a call pickup group can be deleted.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003