BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1030
Public number group

The command is used to assign a trunk to a group of trunks which have all one and the same public number ( e.g a PRA) . The assignment to the group defines which of the 32 public numbers (command 2220 Public number) should be used to create the A/B-number to be sent to the network on request.

Valid data: group 0-group 31

Default data: group 0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003