BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3081
Access to DISA allowed

This command specifies which ACOS (A-categories) are allowed to access the DISA with password control facility.

During login the caller has to identify himself by sending an extension directory number and an authority code. If this data is accepted, the ACOS of the logged-in extension will be checked.

Minimum required authority level from telephone:

Accessible via BMS:

Revision: A © Ericsson Enterprise 2003