BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4004
Cyclical selection

This command is used to state the search principle to be used for the selection of operators.

Y = |  | Sequential search basis - the operator who has been free longest shall be selected

N = |  | Sequential selection - search for a free operator always starts at the first operator in the group. If the first operator is busy, the second will be chosen, and so on.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003