BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0153
Direct carrier access LCR ?

The command defines whether or not the extension is permitted to select a specific carrier by dialling its access code. The call will then not be controlled by LCR functions, day-of-week and time-of-day analysis. LR will however eventually add account- and authority codes according to the carrier definitions.

value =

0 (no): |  | Not allowed to select a carrier directly

1 (yes): |  | Allowed to select a carrier directly

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003