BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2401
Digit for Camp-on

If an extension meets busy on a call to another extension, the calling extension can initiate call waiting by dialling a digit.

This command determines the digit to be used to initiate call waiting.

If the digit is already used for another service, it will be erased for this service, i.e. the “old” service is removed from the system. See other commands in this group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003